

Project’s Report

Project Name:

Vehicle Recognition at Night Based on Tail LightDetection Using Image Processing .

**Submitted To:**

**SUPTA RICHARD PHILIP**

**Lecturer: Dept of CSE**

**Submitted by:**

* Tahamina Afroz Lima
* Id: 161412312
* Sanjida Yasmin
* Id: 161412302

Md.Monirujjaman Sohel Rana

* Id: 161412339
* Alid Hasan Sourav
* Id: 151382316

Contents

Abstrac**t** ------------------------------------ 01

INTRODUCTION----------------------------------------- 01

STATE OF ART ----------------------------------------- 02

METHODOLOGY ----------------------------------------- 04

Circuit ------------------------------------- 08

RESULTS ------------------------------------- 13

CONCLUSION -------------------------------------- 14

REFERENCES ------------------------------------- 14

**Abstract**

Automatic recognition of vehicles in front can be used as a component of systems for forward collisions prevention. When driving in dark conditions, vehicles in front are generally visible by their back lights. Present an algorithm that detects vehicles at night using a camera by searching for tail lights. Develop an image processing systems that can efficiently spot vehicles at different distances and in weather and lightning conditions.

**INTRODUCTION**

Vehicle calamity statistics are jarring at night. Despite 60 percent less traffic on the roads, more Than 40 percent of fatal car accidents occur at night. The statistics for collision are 29 percent of crashes due to collisions in united states of America,18 percent in European Union and 30 percent in Asian countries. In European Union 30 percent and in Asia 60 percent in-vehicle fatalities occurs in darkness. Every year,Thousands of people are injured or killed as a result of vehicle accidents at night time,and in many cases the accident was not the fault of the injured party or the deceased victim.At least 7,221 people were killed and 15,466 others injured in 5,514 road crashes across the country in 2018 [The daily Star], said a passengers' welfare body and At least 7,397 people were killed and 16,193 others injured in 4,979 crashes in 2017 .In developing countries like Bangladesh , fatality rate(defined as,road accidents death per 10,000 vehicles) is quite high in comparison to developed countries. While in Europe and North America the situation is generally improving many developing countries face a worsening situation. Pedestrians and cyclists are often the most vulnerable in night time.The developed countries are now on their way to develop intelligent and smart cars that will help the humanity to avoid accidents during night time detect the vehicle by using their lamp pair,the concepts such as morphological processing and light edge detection are used.these concepts come under Digital Image Processing area .

**STATE OF ART**:

As rear lights must be red by law, several systems have utilizedcolour to aid vehicle detection. Detect rear lights by colour filtering in RGB space to detect red and white regions. If a white region is surrounded for most of its perimeter by red pixels, it is regarded as a potential rear-light. We note that taillights within 40 meters usually appear as white regions in the image as they are too bright for the image sensor. Their white filter was effective, however the red filter allowed through many different colours, resulting in bright objects such as street lamps being let through the filter. The candidates were paired by considering y-values, area and spacing. The RACCOON system uses two thresholds to find tail light pixels, one for brightness and one for redness. Detected tail lights are then tracked using a simple algorithm. The bearing of the target vehicle is estimated by the horizontal position of the centroid of the tail lights.No software signal processing is required. A signal is taken directly from the red channel of the RGB sensor, filtered and thresholded in hardware. This method has a zero processing overhead, but is not adaptable.



Fig. 1.Tail Lights Cause Camera to Saturate in Places

Symmetry is commonly used to filter potential candidates for vehicle detection as the rear of a vehicle is generally symmetrical during daylight and darkness. Some approaches fit an axis of symmetry. While compute intensive, this approach is effective for daylight situations where the scene is more complex than darkness. For detection at night, size and shape of thresholded lights are analyzed. An axis of symmetry is determined, and reflections are distinguished from lights by examining the angle of the axis of symmetry. However this would not be effective from a observation point directly behind and square to the target vehicle. Vertical edges and shadows underneath the vehicle along with symmetry and tail light blobs have been used to detect vehicles by day and night in a particle filter framework .The taillight pairing process can be simplified by making several assumptions. They assume that the average car is around 170cm wide and the width/height aspect ratio of a highway vehicle is approximately 2.0. Morphology has been used to detect vehicle lights. The assumption is made that the lights will be circular or elliptical in shape. However the shape of rear lights is not specified in legislation and automotive designers are experimenting with different shapes as LED lights become more common. A temporal approach can also be used to improve detection rates. To aid detection, the lane ahead can be detected and a mask applied to reduce the area of the image that is searched for target vehicles .

**METHODOLOGY**

Architecture of Proposed Work is given below :



Fig. 2.Architecture of Proposed Work.

A digital camera fitted in the car captures the front vehicles. The input video is of the form mpeg,avi etc. The captured video is converted into number of frames. The numbers of frames are based on the format of the video.For example AVI files 18 Frames/Sec while MPEG requires 26 frames/Sec to avoid loss of information



Fig. 3. Input frame.

1. **Preprocessing** Preprocessing is the process can be carried out into the following list of steps,

– Binarization.

– Noise removal.

In binarization, RGB fames are converted into the binary image. It converts the input image to a binary image. The output image BW replaces all pixels in the input image with luminance greater than level with the value 1 (white) and replaces all other pixels with the value 0 (black).

For removing the noise in the binary image, we calculate the weight of the object. Morphological operation employed here for reduce the noise.In Morphological Operation the technique such as erosion and dilation used.Dilation adds pixels to the boundaries of objects in an image, while erosion removes pixels on object boundaries.The number of pixels added or removed from the objects in an image depends on the size and shape of the structuring Elements used to process the image.Erosion is the processes of removing the noise in the input binary frame. Dilation is the process of reconstructing the interesting region that can be eliminated during the time of noise removal.



Fig. 4.Binary Image

**B. Lamp Edge Detection**

The noise free input frame are subjected into the edge detection.The Edge Detection block finds the edges in an input image by approximating the gradient magnitude of the image. For edge detection, we use the canny edge detector. The canny Edge Detection block finds edges by looking for the local maxima of the gradient of the input image. It calculates the gradient using the derivative of the Gaussian filter. The Canny method uses two thresholds to detect strong and weak edges. It includes the weak edges in the output only if they areconnected to strong edges. As a result, the method is more robust to noise, and more likely to detect true weak edges. The Canny method applies two thresholds to gradients.A high threshold for low edge sensitivity and a low threshold for high edge sensitivity.Edge starts with the low sensitivity result and then grows it to include connected edge pixels from the high sensitivity results this helps fill in gaps in the detected edges. In this case,the contour functions determine the number contours to display based on the minimum and maximum data values.



Fig. 5.lamp Edge Detection

1. **Lamp Pairing**

Pairing based on the size, and intensity of the light objects. the concluding stage in the symmetry check is the comparison of the aspect ratios of the light candidates. This is to prevent objects of different shapes but similar size and position being paired.

**Circuit :**

****

**Fig. 6. Red output from a CCD camera**

Images captured by a CCD camera are easily obtained. We use the red output signal of the three original colors (R, G, and B) from the CCD camera as the input signalfor a voltage comparator to compare with a threshold value. The red output signals of the taillights A and B in relevant scan lines would appear as shown in Fig.6.



Fig. 7.Circuit structure for identifying bright signals

The circuit structure for identifying the red output signal is a simple and practical circuit as shown in Fig.8. The low-pass filter is used to smooth the signals from the CCD, as shown in Fig.6. Because the lights coming from the taillights are not always pure red and affected by other light sources, the threshold value equals the average background signal, which is produced by passing the red output signal R through a low-pass filter, plus a supplemental quantity.We can define different supplemental quantities for different backgrounds. By adjusting the threshold value and supplemental quantity, the proposed measurement system can be applied in various situations .



Fig. 8. Comparator output Rp for identifying the positions of spots A and B.

We can define different supplemental quantities for different backgrounds. By adjusting the threshold value and supplemental quantity, the proposed measurement system can be applied in various situations .The output R of the comparator will produce two positive pulses on a horizontal scanning line as shown in Fig.9. Then,using the two positive pulses as triggers of a counter, the external clock value NK between the two bright spots can be obtained.Given the external clock value, we can transform it to a distance value. From Fig.6, at initialization, we measure the distance between the taillights of a regular car, which constitute the length Dmin, and count the relative interval Nmax. Then, we employ a simple flip-flop, a single-pulse generator, and a counter to obtain Nk. Because DminNmax, and NK are known, we use (1) to get length. If is calculated by (1) and HD is given at initialization, we can use (2) to obtain the actual distance HK. In this brief,we propose a technique for transforming the time value scale into a distance scale that uses a clock counter instead of a pixel counter for measuring the distance between the taillights. This method can enhance measurement speed.

**RESULTS**

This entire process essentially amounts to a symmetry check.If a bounding Box above a certain size is detected then the driver is alerted that a vehicle is close.



Fig. 10.Bounding Box of Detected Image

Bounding boxes resulting from white regions appeared incorrectly,not identifying the target vehicle,4 times in the 200 frames, resulting in a false positive rate of 1.8 percent. These results refer to only a subset of the total video data. The algorithm has demonstrated that it works well in both well lit urban areas and dark rural areas. It also works effectively in wet conditions

**CONCLUSION**

In this paper, we have discussed the need for a system to avoid or mitigate forward collisions during darkness. A background to the relevant automotive rear light legislation, showing characteristics that canbe recognized by image processing, was given. We have presented an algorithm for forward collision detection at night using a visual camera. Our technique filters red and white colours in the HSV colour space. White regions adjacent to red regions are searched for symmetrical pairs, and aspect ratio constraints are applied to resulting bounding boxes. This produces detected rear target vehicle lights. We have shown promising preliminary results, and intend to expand and improve the system. An important next step is to introduce a temporal dimension and track targeted vehicles in video sequences to improve the detection rate, and to detect imminent collisions. It is envisaged to expand the range of test scenarios to make the system more robust .

**REFERENCES**

[1] W.Y.Wang, M.C.Lu, H.L.Kao, and C.Y.Chu. ”Nighttime Vehicle Distance Measuring Systems”. IEEE Transactions on Circuits and Systems II;Express Brifs,54,81-85,2005

[2] Y.-M. Chan, S.-S. Huang, L.-C. Fu, and P.-Y. Hsiao. Vehicle detection under various lighting conditions by incorporating particle filter. In IEEE Intelligent Transporta-tion Systems Conference, pages 534539, 2007.

[3] M. Y. Chern and P. C. Hou. The lane recognition and vehicle detection at night for a camera-assisted car on high-way. Proceedings ICRA03 IEEE International Conference on Robotics and Automation, vol.2, 2003.

[4] R. Cucchiara and M. Piccardi. Vehicle detection under day and night illumination. Proceedings of the 3rd International ICSC Symposia on Intelligent Industrial Automation and Soft computing, pages 14, June 1999.

[5] Y. Du and N. Papanikolopoulos. Real-time vehicle fol-lowing through a novel symmetry-based approach. Pro-ceedings IEEE International Conference on Robotics and Automation, 4:31603165, 1997.

[6] C. Juli‘a, A. Sappa, F. Lumbreras, J. Serrat, and A. Lopez. Motion segmentation from feature trajectories with miss-ing data. In 3rd Iberian Conference on Pattern Recognition and Image Analysis,LNCS vol.1, pp., Girona, Spain, June, 2007.

[7] R. Sukthankar and R. Sukthankar. Raccoon: A real-time autonomous car chaser operating optimally at night. In Intelligent Vehicles 93 Symposium, pages 3742, 1993.

[8] Z. Sun, G. Bebis, and R. Miller. On-road vehicle detection: a review. Transactions on Pattern Analysis and Machine Intelligence, 28:694711, 2006.

[9] R.Taktak,M.Dufaut,andR.Husson.Vehicledetection at nightusingimageprocessingandpatternrecognition. Pro- ceedingsIEEEInternationalConferenceImageProcessing ICIP-94,2,1994

[10] C.-C.Wang,S.-S.Huang,and L.-C.Fu.Driverassistance system forlanedetectionand vehicle recognitionwith night vision. In IEEE/RSJ InternationalConference on IntelligentRobotsandSystems,pages35303535,2005.

[11] W.-Y. Wang, M.-C.Lu,H.L.Kao,andC.-Y.Chu.Night- timevehicledistancemeasuringsystems.IEEETransac- tionsonCircuitsandSystemsII:ExpressBriefs,54:8185,2007

[12] The Daily Star